# Motion Picture and Effects

Log Format • DPX Properties • DPX Settings

DPX (SMPTE 268M-2003) - This format is used in Motion Picture and Effects industry that makes particular use of the extensive header information and the format's flexibility in being able to handle high dynamic range and logarithmic color values at a variety of bit depths using RGB or YCbCr pixel descriptions. It is based on, but largely supersedes, Kodak's Cineon format that has a more film specific header.

One example of it's use includes scanning film for use in post production. Each frame is stored as an individual DPX file ranging from 2k (2048 pixels wide) to 8k (8192 pixels wide - for IMAX frames) at anything between 8 to 64 bits per color component. A sequence of these might then be processed using compositing software, altering the color or adding visual effects. Once complete they might then be recorded digitally to tape or projected back on to film.

The color values for each pixel are often stored logarithmically (particularly if the sequence is destined to be transferred back on to film) which more naturally reflects the density of how color information is stored in the emulsion on the original film. When viewed without alteration, logarithmic files appear to have very low contrast and requires a 'look up table' to translate the logarithmic image to something that resembles what you might see if the image was transferred back to film and projected in a cinema. Apart from making the image linear (like most typical computer images) and adjusting the gamma level this table sets where the black and white point lies.

For a 10 bit logarithmic image where each color component value ranges from 0 to 1023 the black and white points are normally set at 95 for black and 685 for white. What this means is that the logarithmic file stores color values that are lighter than what the linear version will display as pure white and darker than what it will display as pure black. This extra information therefore remains available for an effects artists who might wish to alter the brightness of the image after it has been stored as a DPX file.

As an example, had this information been lost, reducing the brightness of an image uniformly would result in highlights becoming darker, whereas with this extra information the highlights instead reduce in size and start showing details that were previously too bright to be seen. The latter is far closer to what happens in the real world.

The header can contain Film and/or Television specific data related to a production. For example the television header can contain a SMPTE time code so that shots exported as a DPX sequence from a production's edit can be easily replaced once any effects have been added. The film header holds information about the reel of film the frames originated from and various camera settings that were used while filming. All these details usually stay with the images as they are passed between post-production companies.

## Log Format

The color values for each pixel are often stored logarithmically (particularly if the sequence is destined to be transferred back on to film) which more naturally reflects the density of how color information is stored in the emulsion on the original film. When viewed without alteration logarithmic files appear to have very low contrast (leftmost image), and so require a 'look up table' to translate the logarithmic image to something that resembles what you might see if the image was transferred back to film and projected in a cinema (rightmost image). Apart from making the image linear (like most typical computer images) and adjusting the gamma level this table sets where the black and white point lies.

For a 10 bit logarithmic image where each color component value ranges from 0 to 1023 the black and white points are normally set at 95 for black and 685 for white. What this means is that the logarithmic file stores color values that are lighter than what the linear version will display as pure white and darker than what it will display as pure black. This extra information therefore remains available for an effects artists who might wish to alter the brightness of the image after it has been stored as a DPX file.

As an example, had this information been lost, reducing the brightness of a linear image uniformly would result in highlights becoming darker (leftmost image), whereas with this extra information the highlights instead reduce in size and start showing details that were previously too bright to be seen (rightmost image). The latter is far closer to what happens in the real world.

## DPX Properties

ImageMagick supports these DPX properties:

    dpx:file.copyright
    dpx:file.creator
    dpx:file.filename
    dpx:file.project
    dpx:file.version
    dpx:film.count
    dpx:film.format
    dpx:film.frame_id
    dpx:film.frame_position
    dpx:film.frame_rate
    dpx:film.held_count
    dpx:film.id
    dpx:film.offset
    dpx:film.prefix
    dpx:film.sequence_length
    dpx:film.shutter_angle
    dpx:film.slate
    dpx:film.type
    dpx:orientation.aspect_ratio
    dpx:orientation.border
    dpx:orientation.device
    dpx:orientation.filename
    dpx:orientation.serial
    dpx:orientation.x_center
    dpx:orientation.x_offset
    dpx:orientation.x_size
    dpx:orientation.y_center
    dpx:orientation.y_offset
    dpx:orientation.y_size
    dpx:television.black_gain
    dpx:television.black_level
    dpx:television.break_point
    dpx:television.field_number
    dpx:television.frame_rate
    dpx:television.gamma
    dpx:television.integration_times
    dpx:television.interlace
    dpx:television.padding
    dpx:television.time.code
    dpx:television.time_offset
    dpx:television.user.bits
    dpx:television.vertical_sample_rate
    dpx:television.video_signal
    dpx:television.white_level
    dpx:user.id
    dpx:user.data

Look for any user data as the `dpx:user-data` image profile.

To determine which properties are associated with your DPX image, use this command for example:

    identify -verbose bluebells.dpx

To identify a particular property, try this:

    identify -format "%[dpx:television.time.code]" bluebells.dpx

Finally, to set a property:

    convert bluebells.dpx -define dpx:television.time.code=10:00:02:15 bluebells-001.dpx

## DPX Settings

Use -set to specify the image or film gamma or black and white points. For example use:

    -set gamma 1.7
    -set film-gamma 0.6
    -set reference-black 95
    -set reference-white 685
    -set profile dpx:user.data